Probe_Quantities_Enabled

This data set allows the user to link any chosen physical quantity with probes.
The time series of the physical quantity are recorded in a file in ASCII format named n_yyyyy.d, where “n” refers to the name of the physical quantity (i.e. n=u for the i-velocity component, n=t for the temperature, n=r for the density, n= p for the pressure,…). 'yyyyy' is the subdomain number which the probes belong to (particularly useful when the simulation is performed with a MPI domain decomposition approach).
Data are ordered in columns, the first refers to the time, the second refers to the first probe and so on … the position of each probe is written on the first line of each file.

Temporal_Series_For_Quantity_Enabled

Type : Allocatable array of boolean values. The array size is automatically made.

Each array component is associated to a physical quantity in this order :

component of velocity along the I-direction

component of velocity along the J-direction

component of velocity along the K-direction

Temperature

Pressure

Density

Mass fraction of Species 1 (if it exists)

…

Mass fraction of Species n (if it exists)

Each element of the array must be initialized by the values .true. or .false.

The user can activates the chosen physical quantity in order to get time-series related to the probes placed over the domain (see the namelist “Probe_Location”).