Namelist "Field_Recording_Setup"

This data set allows the user

to define the precision (simple or double) on the data related to the instantaneous fields and the statistical fields.

to reduce the dimension of the statistical fields in order to get a profile along a given direction. The reduction is made by space averaging over the other directions.

Full data set of the namelist

&Field_Recording_Setup Precision_On_Instantaneous_Fields= 1, Precision_On_Statistical_Fields= 2 ,
Time_Statistics_Enabled= .true. , Sample_Rate_For_Statistics= 1 ,
Statistic_Space_Average_Type= "NO_SPACE_AVERAGE" /

—–

Precision_On_Instantaneous_Fields

Type : Integer Value

1 : Instantaneous fields are recorded in single precision (r4).

2 : Instantaneous fields are recorded in double precision (r8).

Precision_On_Statistical_Fields

Type : Integer Value

1 : Statistical fields are recorded in single precision (r4).

2 : Statistical fields are recorded in double precision (r8).

Statistic_Profiles

Type : integer value

This data defines the direction in which the profile of a statistical quantity is calculated. A space average is performed over the others directions.

0 : Statistical fields are not reduced in a profile along a specific direction.

1 : The profile is calculated along the I-direction.

2 : The profile is calculated along the J-direction.

3 : The profile is calculated along the K-direction.