Namelist "Slices_Recording_Setup"

This data set is used to define the position and the orientation of a slice on which different instantaneous fields of data will be recorded.

Full data set of the namelist

&Slices_Recording_Setup
Identifier_Value=1, Normal_Direction_Index=1,
Normal_Direction_Coordinate= 0.6 ,
Field_Number= 2,
List_Of_Fields= "U " , "V "/

Identifier_Value

Type : Integer value

Set the ID number of the slice

Normal_Direction_Index

Type : Integer value

Set the normal direction of the slice (I : 1 , J : 2 or K : 3)

Normal_Direction_Coordinate

Type : Real value

Set the position of the slice in the computational domain. The coordinate depends on the orientation of the slice.

Field_Number

Type : Integer value

Set the number of fields to consider.

List_Of_Fields

Type : character string

Set the name of fields to record on the slice (6 characters max.)