Namelist "SpaceAveragedSnapshots_Dataset"

This data set is used to get the space-averaged fields of physical quantities in a specific direction at un given time. The recording rate is specified in the namelist “Simulation_Management”.

Full data set of the namelist

&SpaceAveragedSnapshots_Dataset SpaceAverageDirection="J-DIRECTION", Field_Number=3, List_of_Fields="U","V","W"/

SpaceAverageDirection

Type : Character string

Set the the direction in which the space average is performed : “I-DIRECTION”, “J-DIRECTION” or “K-DIRECTION”

Field_number

Type : Integer value

Set the number of fields for which the space average will be computed.

List_of_Fields

Type : Character string.

Set the name of physical quantities for which the space average will be computed (6 characters max.). See the namelist Namelist "Instantaneous_Fields_Listing" in order to get the list of available physical quantities.