This file is composed with 12 line of integer values.

The first two lines allows the user to select a series of files should be converted. The first line is associated to the subdomain number and the second line to the file number which are included in the file name.

The following line contains one integer value which defines the type of file to convert

0 : instantaneous fields : res_yyyyy_xxxxxxx.d

1 : statistical fields : rst_yyyyy_xxxxxxx.d

The third following lines are associated to the grid indices of the computational domain. These index set allows the user to build a space box for extracting only a part of fields from the computational domain.
If one of these index values is set to zero, the whole domain is considered regardless of the meshsize, including the ghost cells.

The following line contains just one integer value for selecting the type of format in which the file will be converted.
0 : tecplot format (.plt) - 1 : VTK format (.vtk).

The following line is a peculiar data related to the vtk format conversion. An integer data defines if the vtk data must be written as a rectilinear form (value 0) or a structured-grid form (value 1).

The three last lines are reserved to the special case of data manipulation : Please, do not consider them for your work and do not modify them.

00000 1 !--- 1st subdomain number and total number of subdomains for file selection (related to the 1st number in the file name) 0 200 1 !--- 1st file number, last file number and file number-step for file selection (related to the 2nd number in the file name) 0 !--- Type of file to convert (0 : instantaneous fields, 1: statistical fields) 0 130 !--- Start and end indices along the I-direction | => space box for considering only a part of fields 1 130 !--- Start and end indices along the J-direction | a zero value indicates the whole computational domain is considered 1 130 !--- Start and end indices along the K-direction | 1 !--- selection of the format conversion -> 0 : tecplot format (.plt) - 1 : VTK format (.vtk) 0 ! Only for VTK format -> 0 : rectilinear form , 1: structured grid form rst_00000_0000001.d !--- special data. Do not modify it. 0 !--- special data. Do not modify it. 0 !--- special data. Do not modify them. EOF